

**SCHOOL OF PHYSICS**

**UNIVERSITI SAINS MALAYSIA**

**ZCT191/192 PHYSICS PRACTICAL I/II**

**ERROR ANALYSIS**

***Worksheets***

**OBJECTIVES**

1. *To* *understand how to correctly present a physical quantity with its error;*
2. *To estimate the resistivity of a copper wire and its error by measuring its length, resistance and diameter; and*
3. *To study the probability distribution function of the diameter of a copper wire.*

**ERROR ANALYSIS WORKSHEET 1**

*Instructions*: please complete **Worksheet 1** by the end of the first session of your experiment.

Name : TAN WEI LIANG Date : 23-10-2023

Partner’s Name : AINA IMANINA BINTI MOHD KHOZIKIN Group : M5B

**Part A1: Length of a Copper Wire**

**Table 1**: The length of the copper wire.

|  |  |  |  |
| --- | --- | --- | --- |
| **Measurement,** | **Length of wire,**  **0.1** | **(m)** | **()** |
| 1 | 129.5 | -1.875 | 3.51563 |
| 2 | 130.0 | 3.125 | 9.76563 |
| 3 | 129.8 | 1.125 | 1.26563 |
| 4 | 129.7 | 0.125 | 1.56250 |
| 5 | 129.7 | 0.125 | 1.56250 |
| 6 | 129.4 | -2.875 | 8.26562 |
| 7 | 129.7 | 0.125 | 1.56250 |
| 8 | 129.7 | 0.125 | 1.56250 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Sample size, | : | 8 |
|  |  | : | 1.296875 m |
|  |  | : | 0.032678571 |
|  | Standard deviation, | : | 1.807722 m |
|  |  | : | 6.39126 m |
|  | Length of copper wire, | : | 1.2969 0.0006 m |

**Part A2: Resistance of Copper Wire**

**Table 2**: The resistance of the copper wire.

|  |  |  |  |
| --- | --- | --- | --- |
| **Measurement,** | **Resistance of wire,**  **0.1** | **(Ω)** | **()** |
| 1 | 0.8 | -0.05 | 0.0025 |
| 2 | 0.8 | -0.05 | 0.0025 |
| 3 | 0.9 | 0.05 | 0.0025 |
| 4 | 0.8 | -0.05 | 0.0025 |
| 5 | 0.9 | 0.05 | 0.0025 |
| 6 | 0.9 | 0.05 | 0.0025 |
| 7 | 0.8 | -0.05 | 0.0025 |
| 8 | 0.9 | 0.05 | 0.0025 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Sample size, | : | 8 |
|  |  | : | 0.850 Ω |
|  |  | : | 0.002857143 |
|  | Standard deviation, | : | 0.053452248 Ω |
|  |  | : | 0.018898224 Ω |
|  | Resistance of copper wire, | : | 0.85 0.02 Ω |

**Part A3: Diameter of Copper Wire**

**Table 3**: The diameter of the copper wire.

|  |  |  |  |
| --- | --- | --- | --- |
| **Measurement,** | **Diameter of wire,** | **(m)** | **()** |
| 1 | 0.21 | 2.5 | 6.25 |
| 2 | 0.23 | 2.25 | 5.0625 |
| 3 | 0.20 | -7.5 | 5.625 |
| 4 | 0.19 | -1.75 | 3.0625 |
| 5 | 0.17 | -3.75 | 1.40625 |
| 6 | 0.23 | 2.25 | 5.0625 |
| 7 | 0.20 | -7.5 | 5.625 |
| 8 | 0.23 | 2.25 | 5.0625 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Zero error | : | 0 m |
|  | Sample size, | : | 8 |
|  |  | : | 2.075 m |
|  |  | : | 4.78571 |
|  | Standard deviation, | : | 2.18763 m |
|  |  | : | 7.73443 m |
|  | Diameter of copper wire, | : | (2.0750.077) m |
|  | Diameter of copper wire (lab reference book), | : | 1.93 m |
|  |  | : | 7.51 % |

**Analysis**

Fill in the blanks with the correct answers, uncertainties and units.

The measured values of the length (), resistance () and diameter () of the SWG36 copper wire are

m

0.85 ± 0.02 Ω

(2.075 0.077) m

The best estimate of the resistivity of the copper wire is .  
*[Show your calculations in the space provided below. Use the correct units in your final answer.]*

|  |
| --- |
|  |

The uncertainty of the resistivity of the copper wire is 1.95 .

*[Show your calculations in the space below. Hint: use the variance formula from the guidebook.]*

|  |
| --- |
| 1.725623915 |

The final estimated resistivity of the SWG36 copper wire is therefore   
.

The temperature in the first-year lab is .

The standard values of the resistivity for the SWG36 copper wire SWG 36 at different temperatures are

Plot of vs. :

|  |
| --- |
|  |

**Figure 1**: Plot of vs. .

From the graph, the estimated standard resistivity of a copper wire at laboratory temperature is .

The percentage discrepancy between the standard resistivity and the experimental resistivity of the copper wire is 28.31 %.

*[Show your calculations in the space below, and comment if your result is accurate.]*

|  |
| --- |
| percentage discrepancy,  Since the percentage of discrepancy is large, the standard resistivity and the experimental resistivity of the copper wire are not consistent and indicated the presence of systematic error. |

1. The sources of systematic errors observed in this experiment are:

*[Comment if they are significant.]*

|  |
| --- |
| The length of the copper wire is influenced by changes in surrounding temperature, causing linear expansion. This statement suggests that temperature can affect the length of the copper wire. This is a systematic error because it consistently influences measurements in a specific way.  The multimeter lacks the necessary sensitivity to detect small changes in resistance and offers limited resolution. This is a systematic error because it consistently affects the measurements by limiting the precision and sensitivity of the equipment.  Inconsistencies in enamel coating removal, if the process of removing enamel coating from the copper wire is not done consistently across all measurements or if it inadvertently damages the wire. This is a systematic error because it consistently affects the measurements by the copper wire is not done consistently across all measurements. |

1. Other sources of errors in this experiment include:

*[List down at least three sources, and explain briefly how these errors affected your results.]*

|  |
| --- |
| When data falls between the smallest division on the micrometre scale, it can be challenging to accurately determine the nearest value, especially for individuals with poor eyesight. This is not a systematic error. It's more related to the experimenter's limitations and doesn't consistently affect measurements in the same way. It's more of a random error.  During length measurements, the copper wire may not be perfectly aligned or straight, which can introduce errors in the data. This is not a systematic error. It's more related to the setup and handling of the experiment, leading to random errors.  The resistivity-temperature graph is not necessarily linear in theoretical models, and the provided standard values for SWG36 copper resistivity may lack the necessary information to represent real-world results for data analysis. This is not a systematic error. It's related to the theoretical understanding and the accuracy of the provided resistivity data, but it doesn't consistently affect measurements in the same way.  When the copper wire is sanded, it generates heat, raising the temperature and subsequently increasing resistance. Immediate resistance measurements using a multimeter in this scenario can yield inaccurate data. This is not a systematic error. It's more related to the timing and procedure of measurements and introduces a random error due to the delay between sanding and measurement. |

1. The fractional uncertainty of the measured resistivity of the SWG36 copper wire is 7.66 %.

*[Show your calculations in the space below, and comment if your result is precise.]*

|  |
| --- |
| Fractional uncertainty,      Since the fractional uncertainty is small, the result of measurement is precise. |

1. The precision of the resistivity measurement can improve if

*[List down at least three suggestions.]*

|  |
| --- |
| The temperature of labs is set as constant temperature to avoid the linear expansion of copper wire. The measuring apparatus in smaller scale division or more sensitivity is suggested to use in measurement. When using a multimeter for measurement, ensure that the probes are clamped properly and tightly onto the copper wire.  During sanding the copper wire, must be sanding gently and stop immediately when observed the shiny surface is formed to avoid over sanding. After sanding the surface layer of wire, it should be wait until the friction-generated temperature drops to lab temperature before measurement. After sanding, the copper must always keep in straight to avoid the deformation of the cross-sectional area when it was bent before the measurement of diameter. The copper wire should always be kept straight when taking measurements to obtains accurate length.  The more larger sample size is suggested to take in experiment for the more accuracy average results and smaller standard error. |

**Conclusion**

1. The resistivity of the copper wire at temperature26.0 is .
2. The agreement between experimental and standard values is ~~good~~ / not good\*. The systematic errors are significant / ~~insignificant~~\*.

*[\*Strike out whichever is not applicable.]*

**ERROR ANALYSIS WORKSHEET 2**

*Instructions*: please complete **Worksheet 2** by the end of the second session of your experiment.

Name : TAN WEI LIANG Date : 30-10-2023

Partner’s Name : AINA IMANINA BINTI MOHD KHOZIKIN Group : M5B

**Data**

**Table 4**: Diameter () measurements of the copper wire for samples to 40. Students are required to obtain three samples of readings only, as the remaining 37 samples have been provided for you.

|  |  | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **1** | **2** | **3** | **4** | **5** | **6** | **7** | **8** |
| **1** | 220 | 190 | 190 | 200 | 200 | 190 | 200 | 200 |
| **2** | 190 | 190 | 190 | 190 | 190 | 210 | 190 | 190 |
| **3** | 190 | 190 | 190 | 190 | 190 | 190 | 190 | 190 |
| **4** | 196 | 206 | 191 | 193 | 192 | 190 | 195 | 193 |
| **5** | 197 | 193 | 193 | 198 | 188 | 191 | 191 | 195 |
| **6** | 203 | 201 | 196 | 195 | 196 | 197 | 193 | 189 |
| **7** | 201 | 205 | 203 | 197 | 196 | 189 | 197 | 200 |
| **8** | 200 | 195 | 193 | 196 | 201 | 188 | 196 | 195 |
| **9** | 195 | 201 | 206 | 198 | 196 | 194 | 189 | 198 |
| **10** | 194 | 198 | 199 | 198 | 196 | 206 | 196 | 198 |
| **11** | 201 | 199 | 193 | 191 | 190 | 189 | 190 | 188 |
| **12** | 192 | 190 | 191 | 197 | 190 | 189 | 193 | 188 |
| **13** | 197 | 198 | 200 | 199 | 206 | 198 | 195 | 200 |
| **14** | 191 | 190 | 198 | 196 | 196 | 201 | 196 | 196 |
| **15** | 194 | 205 | 202 | 203 | 197 | 191 | 193 | 199 |
| **16** | 199 | 195 | 198 | 199 | 205 | 206 | 208 | 192 |
| **17** | 204 | 196 | 199 | 199 | 192 | 193 | 196 | 197 |
| **18** | 193 | 200 | 191 | 191 | 192 | 199 | 203 | 198 |
| **19** | 196 | 193 | 193 | 203 | 205 | 194 | 194 | 199 |
| **20** | 199 | 193 | 195 | 188 | 199 | 199 | 197 | 190 |
| **21** | 197 | 194 | 191 | 195 | 195 | 195 | 203 | 206 |
| **22** | 197 | 196 | 200 | 197 | 198 | 195 | 194 | 195 |
| **23** | 190 | 197 | 189 | 195 | 193 | 195 | 197 | 189 |
| **24** | 195 | 197 | 196 | 199 | 205 | 195 | 198 | 196 |
| **25** | 191 | 194 | 197 | 198 | 199 | 200 | 199 | 194 |
| **26** | 201 | 193 | 196 | 197 | 192 | 196 | 198 | 198 |
| **27** | 191 | 197 | 195 | 196 | 187 | 195 | 197 | 202 |
| **28** | 197 | 197 | 193 | 201 | 195 | 193 | 193 | 193 |
| **29** | 196 | 193 | 199 | 199 | 191 | 195 | 191 | 195 |
| **30** | 203 | 206 | 195 | 195 | 189 | 195 | 197 | 195 |
| **31** | 193 | 203 | 201 | 201 | 195 | 205 | 196 | 199 |
| **32** | 196 | 192 | 196 | 201 | 195 | 196 | 197 | 196 |
| **33** | 196 | 195 | 197 | 198 | 195 | 197 | 199 | 195 |
| **34** | 200 | 196 | 206 | 193 | 195 | 192 | 198 | 192 |
| **35** | 196 | 201 | 196 | 199 | 193 | 201 | 197 | 209 |
| **36** | 196 | 195 | 195 | 195 | 196 | 198 | 197 | 195 |
| **37** | 197 | 195 | 194 | 196 | 196 | 200 | 198 | 198 |
| **38** | 193 | 194 | 190 | 193 | 194 | 190 | 196 | 195 |
| **39** | 195 | 197 | 195 | 199 | 193 | 196 | 193 | 213 |
| **40** | 192 | 196 | 193 | 192 | 196 | 199 | 198 | 194 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Sample size, | : | 320 |
|  |  | : | 1.96025  m |
|  |  | : | 2.1084 |
|  | Standard deviation, | : | 4.591731699 m |
|  |  | : | 2.566856053 m |
|  | Diameter of copper wire, | : | (1.960 0.003) m |

**Table 5**: The frequency distribution for the diameter readings of the copper wire.

|  |  |  |
| --- | --- | --- |
| **Bin Ranges ()**  **[E.g. 185.5 – 187.5]** | **Number of Readings,** | **Ratio,**  **(Total Sample Size, 320\_)** |
| 184.5-186.5 | 0 | 0 |
| 186.5-188.5 | 6 | 0.01875 |
| 188.5-190.5 | 36 | 0.1125 |
| 190.5-192.5 | 25 | 0.078125 |
| 192.5-194.5 | 42 | 0.13125 |
| 194.5-196.5 | 81 | 0.253125 |
| 196.5-198.5 | 51 | 0.159375 |
| 198.5-200.5 | 36 | 0.1125 |
| 200.5-202.5 | 15 | 0.046875 |
| 202.5-204.5 | 9 | 0.028125 |
| 204.5-206.5 | 14 | 0.04375 |
| 206.5-208.5 | 1 | 0.003125 |
| 208.5-210.5 | 2 | 0.00625 |
| 210.5-212.5 | 0 | 0 |
| 212.5-214.5 | 1 | 0.003125 |
| 214.5-216.5 | 0 | 0 |
| 216. 5-218.5 | 0 | 0 |
| 218.5-220.5 | 1 | 0.003125 |

|  |
| --- |
|  |

**Figure 2**: Histogram of vs. .

**Analysis**

1. The maximum point of the histogram is located at 1.955, with a value of 0.253.
2. The percentage difference between and is 0.26 %.

*[Show your calculations in the space below, and comment if your results are consistent with each other.]*

|  |
| --- |
| percentage difference,  Since, the percentage difference is small, both result of diameter is consistent. The percentage difference is smaller than 1.0% indicated the results are very closer. |

1. The area under the Gaussian curve is 2.00m.

*[Show your workings below.]*

|  |
| --- |
|  |

1. The standard deviation () of the sketched Gaussian curve is.

*[Show all the steps that you have used to obtain the answer.]*

|  |
| --- |
|  |

1. The percentage difference between the standard deviation obtained using statistical analysis () and the standard deviation obtained using a best-fit Gaussian curve () is .

*[Show your calculations in the space below, and comment if your results are consistent with each other. Determine which is a more appropriate standard deviation for the diameter of the copper wire, and if the sample distribution approximates a Gaussian distribution well.]*

|  |
| --- |
| percentage discrepancy,  Since the percentage difference is large, both results are not consistent. For achieving accuracy, the method in step 4 is the preferred method in comparison to that of step 3. The calculation of area under the curve through grid-based measurements on graph paper is susceptible to imperfections and inaccuracies, leading to a greater error. in contrast, the method relying on equations to compute standard deviation is favoured for its reduced reliance on approximation variables, thereby enhancing its accuracy. |

In a normal experiment, you will not have sufficient time to collect 40 sets of data with 8 readings for each set to make the above estimation of mean and standard deviation. Usually, only one set of data is obtained, and all the errors will be estimated from this set of data.

1. Taking only data from sample from **Table 4**, The best estimate of the diameter of the copper wire is , which is within 1.39% percentage difference from calculated using all 40 samples.

*[Show your workings below, and comment if both results are consistent with one another.]*

|  |
| --- |
| percentage difference,  Since the percentage of difference is 1.39%, both results are consistent. |

1. The fractional uncertainties of and are 1.84 % and 0.15 %, respectively.

*[Show your workings below, and determine which measurement is more precise.]*

|  |
| --- |
| Fractional uncertainty,  Fractional uncertainty,  the fractional uncertainties of is smaller than indicate the measurements conducted in Part B yielded more precise results. |

1. By using the value of calculated using all 40 samples, and the values of and calculated in **Part A**, the best estimate of the resistivity of the copper wire is   
    .

*[Show all the steps that you have used to obtain the answer.]*

|  |
| --- |
|  |

1. By using and obtained in **Part A** as well as obtained in **Part B**, the uncertainty of the resistivity of the copper wire is 4.693.

*[Show all the steps that you have used to obtain the answer.]*

|  |
| --- |
| 4.693024893 |

1. The final estimated resistivity of the SWG36 copper wire at temperature 26.0 is ( ).
2. The percentage difference between the resistivity obtained in **Part A** and **Part B** is.

*[Show your workings below, and comment if the results are consistent with each other.]*

|  |
| --- |
| percentage difference,  The presence of large percentage difference suggests two results are not consistent.  Given that the sample size in Part B of 320 is larger than that in Part A of 8, the standard resistivity value obtained in Part B is considered more accurate in comparison to that in Part A. Consequently, a significant and large discrepancy is observed. |

1. From **Figure 1**, the standard resistivity value for the SWG36 copper wire at the same temperature is , which is within percentage discrepancy with the results obtained in **Part B**.

*[Show your workings below, and comment if your result is accurate.]*

|  |
| --- |
| percentage discrepancy,  The large percentage discrepancy, exceeding 10%, indicates a significant inconsistency between the two results. |

**Conclusion**

1. The resistivity of the copper wire at temperature 26.0 is ( ).
2. The percentage discrepancy between the standard and measured values of is significant / ~~insignificant~~\*.

*[\*Strike out whichever is not applicable.]*

**ABSTRACT**

The title of this experiment is Error Analysis. This physics experiment delves into the comprehensive study of error analysis during the measurement of the resistivity of copper wire. Employing error propagation techniques and statistical analysis of wire diameters, the objective is to gain a profound understanding of correctly present a physical quantity along with its associated error, and estimating the resistivity of a copper wire, along with its error, through the measurement of length, resistance, and diameter. Additionally, the experiment explores the probability distribution function of the diameter of a copper wire. The experiment is divided into two parts: Part A and Part B. In Part A, the measurement of length, resistance, and diameter of SWG 36 copper wire is utilized to calculate the resistivity, resulting in a value of From the graph, the estimated standard resistivity of a copper wire at laboratory temperature is 1.73 at temperature 26.0 .The experiment reveals a 28.31% percentage discrepancy between the standard and experimental resistivity, indicating significant systematic errors. The agreement between experimental and standard values is not good. The systematic errors are significant in part A. In Part B, the diameter of SWG 36 copper wire is determined from a sample size of 320, and errors are estimated using statistical analysis. The experiment demonstrates that the method for obtaining standard deviation through a best-fit Gaussian curve is more precise than traditional statistical analysis. The resistivity of the copper wire is determined as ( ) , with a 14.45% percentage discrepancy between the standard and measured values. The percentage discrepancy between the standard and measured values of ρ is also significant in part B. In conclusion, this experiment highlights the inevitability of uncertainties and errors in measurements, as well as the importance of precise analysis methods, and emphasizes the need for meticulous error analysis in physical experiments.